; Windows 98SE/ME USB Modem Setup File

; Copyright (c) 2005 Motorola

; Manufacturer: Motorola

; Revision History :

;

; LIBdd18138 - PID change for Talon Int.

; LIBdd25316 - Support for Qualcomm 6050 chipset

; LIBdd73554   2-3-2004  Support for QualComm 6100 and 6300 chipsets
;1/11/2005 -Added support for the E815(Hollywood) CDMA/1X 6500 chipset
;1/11/2005 -Added support for the C364 idProduct: 0x2A82

[Version]

CatalogFile=mdmluc.cat

LayoutFile=layout.inf,layout1.inf,layout2.inf

Signature="$CHICAGO$"

Class=Modem

Provider=%Motorola%

CLASSGUID={4D36E96D-E325-11CE-BFC1-08002BE10318}

DriverVer=1/11/2005, 2.0.0.6


[Manufacturer]

%Motorola%=Motorola



[Motorola]

%USBCDMA%    		= USBCDMA,    USB\MOTUSBCDMA

%USBPATRIOT% 		= USBPATRIOT, USB\MOTUSBPATRIOT

%USBLCA% 		= USBLCA,  USB\MOTUSBLCA

%USB1XCDMA%		= USB1XCDMA,  USB\MOTUSB1XCDMA

%USB1XCDMA5100% 	= USB1XCDMA5100,  USB\MOTUSB1XCDMA5100

%USBTALON% 		= USBTALON,  USB\MOTUSBTALON

%USBTALONINT% 		= USBTALONINT,  USB\MOTUSBTALONINT

%USBHELEN%		= USBHELEN,  USB\MOTUSBHELEN

%USBNEPTUNEULS%		= USBNEPTUNEULS, USB\MOTUSBNEPTUNEULS

%USBNEPTUNELTS%		= USBNEPTUNELTS, USB\MOTUSBNEPTUNELTS

%USBEZX%		= USBEZX, USB\MOTUSBEZX

%USBNEPTUNELTE%		= USBNEPTUNELTE, USB\MOTUSBNEPTUNELTE

%USBNEPTUNELTX%		= USBNEPTUNELTX, USB\MOTUSBNEPTUNELTX

%USBQUALCOMM6050%	= USBQUALCOMM6050, USB\MOTUSBQUALCOMM6050

%USBMSM6100%            = USBMSM6100,USB\MOTUSBMSM6100
%USBMSM6300%            = USBMSM6300,USB\MOTUSBMSM6300
%USBMSM6500%            = USBMSM6500,USB\MOTUSBMSM6500
%USBMSMC364%            = USBMSMC364,USB\MOTUSBMSMC364

[USBCDMA]

AddReg = All, MDMsettings, MDMresponses, CDMAspecific



[USBPATRIOT]

AddReg = All, MDMsettings, MDMresponses



[USBLCA]

AddReg = All, MDMsettings, MDMresponses



[USB1XCDMA]

AddReg = All, MDMsettings, MDMresponses



[USB1XCDMA5100]

AddReg = All, MDMsettings, MDMresponses



[USBTALON]

AddReg = All, MDMsettings, MDMresponses



[USBTALONINT]

AddReg = All, MDMsettings, MDMresponses



[USBHELEN]

AddReg = All, MDMsettings, MDMresponses



[USBNEPTUNEULS]

AddReg = All, MDMsettings, MDMresponses



[USBNEPTUNELTS]

AddReg = All, MDMsettings, MDMresponses



[USBEZX]

AddReg = All, MDMsettings, MDMresponses



[USBNEPTUNELTE]

AddReg = All, MDMsettings, MDMresponses



[USBNEPTUNELTX]

AddReg = All, MDMsettings, MDMresponses



[USBQUALCOMM6050]

AddReg = All, MDMsettings, MDMresponses



[USBMSM6100]
AddReg = All, MDMsettings, MDMresponses

[USBMSM6300]
AddReg = All, MDMsettings, MDMresponses

[USBMSM6500]
AddReg = All, MDMsettings, MDMresponses

[USBMSMC364]
AddReg = All, MDMsettings, MDMresponses

[All]

HKR,,FriendlyDriver,,unimodem.vxd

HKR,,DevLoader,,*vcomm

HKR,,ConfigDialog,,modemui.dll

HKR,,EnumPropPages,,"modemui.dll,EnumPropPages"

HKR,,PortSubClass,1,02

HKR,,DeviceType,1,01

HKR,,PortDriver,,wdmmdmld.vxd

HKR,,Contention,,



[MDMsettings]

HKR,, Properties, 1, 08,01,00,00, FF,00,00,00, FF,00,00,00, 07,00,00,00, 0F,00,00,00, F7,03,00,00, 00,C2,01,00, C0,DA,00,00

HKR,, InactivityScale, 1, 3c,00,00,00

HKR, Init,      1,, "AT<cr>" 

HKR, Init,      2,, "ATE1V1&D2<cr>"

HKR, Answer,    1,, "ATA<cr>"

HKR, Hangup,    1,, "ATHE1<cr>"

HKR,, Reset,, "AT<cr>"   

HKR, Settings, Prefix,, "AT"

HKR, Settings, Terminator,, "<cr>"

HKR, Settings, DialPrefix,, "D"

HKR, Settings, DialSuffix,, ""

HKR, Settings, Tone,, "T"

HKR, Monitor, 1,, "ATS0=0<cr>"

HKR, Monitor, 2,, "None"

HKR, Settings, FlowControl_Off,,  "+IFC=0,0"

HKR, Settings, FlowControl_Hard,, "+IFC=2,2"

HKR, Settings, FlowControl_Soft,, "+IFC=1,1"



[MDMresponses]

HKR, Responses, "0<cr>",  1, 00, 00, 00,00,00,00, 00,00,00,00 ; OK - Command executed

HKR, Responses, "1<cr>",  1, 02, 00, 00,00,00,00, 00,00,00,00 ; CONNECT - Connection

HKR, Responses, "2<cr>",  1, 08, 00, 00,00,00,00, 00,00,00,00 ; RING - Ring signal indicated

HKR, Responses, "3<cr>",  1, 04, 00, 00,00,00,00, 00,00,00,00 ; NO CARRIER 

HKR, Responses, "4<cr>",  1, 03, 00, 00,00,00,00, 00,00,00,00 ; ERROR - Invalid command

HKR, Responses, "6<cr>",  1, 05, 00, 00,00,00,00, 00,00,00,00 ; NO DIALTONE - No dial tone detected

HKR, Responses, "7<cr>",  1, 06, 00, 00,00,00,00, 00,00,00,00 ; BUSY - Engaged (busy) signal

HKR, Responses, "8<cr>",  1, 07, 00, 00,00,00,00, 00,00,00,00 ; NO ANSWER

HKR, Responses, "<cr><lf>OK<cr><lf>",                1, 00, 00, 00,00,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>RING<cr><lf>",              1, 08, 00, 00,00,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>ERROR<cr><lf>",             1, 03, 00, 00,00,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>NO DIALTONE<cr><lf>",       1, 05, 00, 00,00,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>NO DIAL TONE<cr><lf>",      1, 05, 00, 00,00,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>BUSY<cr><lf>",              1, 06, 00, 00,00,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>NO CARRIER<cr><lf>",        1, 04, 00, 00,00,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>NO ANSWER<cr><lf>",         1, 07, 00, 00,00,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT<cr><lf>",           1, 02, 00, 00,00,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 300<cr><lf>",       1, 02, 00, 2C,01,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 600<cr><lf>",       1, 02, 00, 58,02,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 1200<cr><lf>",      1, 02, 00, B0,04,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 2400<cr><lf>",      1, 02, 00, 60,09,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 4800<cr><lf>",      1, 02, 00, C0,12,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 7200<cr><lf>",      1, 02, 00, 20,1C,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 9600<cr><lf>",      1, 02, 00, 80,25,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 12000<cr><lf>",     1, 02, 00, E0,2E,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 14400<cr><lf>",     1, 02, 00, 40,38,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 16800<cr><lf>",     1, 02, 00, A0,41,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 19200<cr><lf>",     1, 02, 00, 00,4B,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 21600<cr><lf>",     1, 02, 00, 60,54,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 24000<cr><lf>",     1, 02, 00, C0,5D,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 26400<cr><lf>",     1, 02, 00, 20,67,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 28800<cr><lf>",     1, 02, 00, 80,70,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 31200<cr><lf>",     1, 02, 00, e0,79,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 33600<cr><lf>",     1, 02, 00, 40,83,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 38400<cr><lf>",     1, 02, 00, 00,96,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 57600<cr><lf>",     1, 02, 00, 00,E1,00,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 115200<cr><lf>",    1, 02, 00, 00,C2,01,00, 00,00,00,00

HKR, Responses, "<cr><lf>CONNECT 115,200<cr><lf>",   1, 02, 00, 00,C2,01,00, 00,00,00,00



[CDMAspecific]

HKR, Fax, FixModemClass,, "2.0"

HKR, Fax, HardwareFlowControl,, "1"



[Strings]

Motorola="Motorola"

USBCDMA="Motorola USB Modem"

USBPATRIOT="Motorola USB Modem"

USBLCA="Motorola USB Modem" 

USB1XCDMA="Motorola USB Modem" 

USB1XCDMA5100="Motorola USB Modem" 

USBTALON="Motorola USB Modem" 

USBTALONINT="Motorola USB Modem" 

USBHELEN="Motorola USB Modem" 

USBNEPTUNEULS="Motorola USB Modem"

USBNEPTUNELTS="Motorola USB Modem"

USBEZX="Motorola USB Modem"

USBNEPTUNELTE="Motorola USB Modem"

USBNEPTUNELTX="Motorola USB Modem"

USBQUALCOMM6050="Motorola USB Modem"

USBMSM6100="Motorola USB Modem"
USBMSM6300="Motorola USB Modem"
USBMSM6500="Motorola USB Modem"
USBMSMC364="Motorola USB Modem"
